[Main]
FileType=CIR
Version=9.00
Program=Micro-Cap
Screen=1280,1024
MCAPVersion=9.0.1.0
Key ID=208 332 945
NLCnt=93
TXCnt=15

[shapedef]
Name=Battery
Line=0,0,22,0
Line=22,-3,22,3
Line=26,-7,26,7
Line=26,0,48,0
Current=32,8,16,8

[shapedef]
Name=SPICE_V
Root="Vsource.root",0,-12,0

[shapedef]
Name=Resistor
PolyOpen=12 
PolyLine=0,0
PolyLine=0,0
PolyLine=12,0
PolyLine=14,-4
PolyLine=18,4
PolyLine=22,-4
PolyLine=26,4
PolyLine=30,-4
PolyLine=34,4
PolyLine=36,0
PolyLine=48,0
PolyLine=48,0
Current=32,8,16,8

[shapedef]
Name=Capacitor
Line=0,0,22,0
Line=22,-8,22,8
Line=26,-8,26,8
Line=26,0,48,0
Current=32,12,16,12

[shapedef]
Name=Inductor
Line=42,0,48,0
Line=0,0,5,0
Arc=5,-7,17,7 , 11,-7,5,0
Arc=13,-7,25,7 , 19,-7,13,0
Arc=29,-7,41,7 , 35,-7,29,0
Arc=21,-7,33,7 , 27,-7,21,0
Arc=6,-7,18,7 , 18,0,12,-7
Arc=14,-7,26,7 , 26,0,20,-7
Arc=22,-7,34,7 , 34,0,28,-7
Arc=30,-7,42,7 , 42,0,36,-7
Line=11,-7,12,-7
Line=19,-7,20,-7
Line=27,-7,28,-7
Line=35,-7,36,-7
Arc=13,-4,17,2 , 13,-1,15,2
Arc=29,-4,33,2 , 29,-1,31,2
Arc=21,-4,25,2 , 21,-1,23,2
Arc=14,-4,18,2 , 16,2,18,-1
Arc=30,-4,34,2 , 32,2,34,-1
Arc=22,-4,26,2 , 24,2,26,-1
Line=15,2,16,2
Line=23,2,24,2
Line=31,2,32,2
Line=5,5,9,5
Line=41,5,41,9
Line=39,7,43,7
Current=32,8,16,8

[shapedef]
Name=Diode
Root="Diode.root",0,-8,0

[shapedef]
Name=Opamp
Root="Opamp.root",0,-4,0

[shapedef]
Name=NFV
Root="Vsource.root",0,-12,0
Root="TextN.Root",20,-6,1
Root="TextF.Root",20,1,1

[shapedef]
Name=NFI
Root="Isource.Root",-12,0,0
Root="TextN.Root",-26,20,0
Root="TextF.Root",-18,20,0

[shapedef]
Name=Or2
Root="Or.root",0,-18,0

[shapedef]
Name=Ground
Line=0,0,12,0
Line=12,-8,12,8
Line=18,-4,18,4
Line=24,0,24,0

[shapedef]
Name=Switch
Line=0,0,0,0
Line=0,48,0,48
Line=48,0,48,16
Line=48,48,48,24
Line=48,16,52,20
Root="Plus.root",6,6,0
Root="Minus.root",6,40,0
Ellipse=-2,-2,2,2
Ellipse=-2,46,2,50

[shapedef]
Name=Diode.root
Line=0,0,20,0
Line=28,0,48,0
Rectangle=18,-8,20,8,SOLID
PolyClosed=3 ,Solid
PolyLine=20,0
PolyLine=28,-8
PolyLine=28,8
Current=32,16,16,16

[shapedef]
Name=Opamp.root
Line=0,48,6,48
Line=0,0,5,0
Line=6,-4,6,52
Line=6,-4,48,24
Line=6,52,48,24
Line=48,24,72,24
Line=10,12,14,12
Line=12,10,12,14
Line=10,36,14,36
Line=4,0,6,0

[shapedef]
Name=Minus.root
Line=-2,0,2,0

[shapedef]
Name=Vsource.root
Line=0,0,12,0
Line=36,0,48,0
Ellipse=12,-12,36,12
Line=7,5,7,9
Root="Plus.root",39,5,0
Current=32,16,16,16

[shapedef]
Name=Or.root
Line=42,8,48,8
Line=0,0,10,0
Line=0,16,10,16
Line=24,-4,6,-4
Line=6,20,24,20
Arc=5,-4,43,34 , 42,8,24,-4
Arc=0,-4,12,20 , 6,20,6,-4
Arc=5,-18,43,20 , 24,20,42,8

[shapedef]
Name=Plus.root
Line=-2,0,2,0
Line=0,-2,0,2

[shapedef]
Name=TextF.Root
Line=0,0,5,0
Line=0,0,0,8
Line=2,4,0,4

[shapedef]
Name=Isource.Root
Ellipse=-12,12,12,36
Line=0,0,0,24
PolyClosed=3 ,Solid
PolyLine=-4,24
PolyLine=4,24
PolyLine=0,32
Line=0,32,0,48
Current=16,16,16,32

[shapedef]
Name=TextN.Root
Line=0,8,0,0
Line=0,0,5,8
Line=5,8,5,0

[shapedef]
Name=Fflop
Text="S",13,-5,21,6 , -9,0,"Arial"
Text="Q",45,-5,54,6 , -9,0,"Arial"
Text="Qb",42,19,56,30 , -9,0,"Arial"
Text="R",13,19,22,30 , -9,0,"Arial"
Rectangle=8,-8,56,32
Line=0,0,8,0
Line=0,24,8,24
Line=64,0,56,0
Line=64,24,56,24

[compdef]
Name=Battery
Definition=Battery
Shape=Battery
Mask=4865
memo=Battery
Label Offset=19,7,10,13
PinCnt=2
Pin="Plus",6,0,-4,-5
Pin="Minus",0,0,-10,-5

[compdef]
Name=Ground
Definition=Ground
Shape=Ground
Mask=1793
memo=Ground
Label Offset=0,0,0,0
PinCnt=1
Pin="PinA",0,0,-3,-7

[compdef]
Name=S (V-Switch)
Definition=S
Shape=Switch
Mask=4096
memo=Voltage Controlled Switch
Label Offset=56,9,-27,51
PinCnt=4
Pin="Plus Output",6,0,-3,-3
Pin="Minus Output",6,6,-5,20
Pin="Plus Control",0,0,-33,-3
Pin="Minus Control",0,6,-41,20

[compdef]
Name=Resistor
Definition=Resistor
Shape=Resistor
Mask=7937
memo=Resistor
Label Offset=18,6,8,11
PinCnt=2
Pin="Plus",6,0,-10,-4
Pin="Minus",0,0,-14,-4

[compdef]
Name=Fflop
Definition=Subckt
Shape=Fflop
Mask=6016
memo=SR Flip-Flop - Christophe Basso model for SMPS testing
Label Offset=27,34,11,17
PinCnt=4
Pin="6",a,0,0,-3,-2
Pin="8",a,0,3,-3,-2
Pin="2",a,8,0,-2,-2
Pin="1",a,8,3,-2,-2

[compdef]
Name=Voltage Source
Definition=VSpice
Shape=SPICE_V
Mask=4864
memo=Voltage Source
Label Offset=19,13,15,13
PinCnt=2
Pin="Plus",6,0,-5,-6
Pin="Minus",0,0,-20,-6

[compdef]
Name=OR2_CB
Definition=Subckt
Shape=Or2
Mask=4992
memo=OR2 - Christophe Basso model for SMPS testing
Label Offset=15,21,6,9
PinCnt=3
Pin="1",a,0,0
Pin="2",a,0,2
Pin="3",a,6,1

[compdef]
Name=Diode
Definition=Diode
Shape=Diode
Mask=5889
memo=Diode
Label Offset=17,10,12,12
PinCnt=2
Pin="Anode",6,0,-9,-8
Pin="Cathode",0,0,-20,-8

[compdef]
Name=Inductor
Definition=Inductor
Shape=Inductor
Mask=7681
memo=Inductor
Label Offset=18,9,11,12
PinCnt=2
Pin="Plus",6,0,-5,-9
Pin="Minus",0,0,-3,-9

[compdef]
Name=Capacitor
Definition=Capacitor
Shape=Capacitor
Mask=6913
memo=Capacitor
Label Offset=16,12,12,12
PinCnt=2
Pin="Plus",6,0,-3,-5
Pin="Minus",0,0,-14,-5

[compdef]
Name=AMPSIMP
Definition=Subckt
Shape=Opamp
Mask=4608
memo=Basso Simple Amplifier
Label Offset=30,39,-6,25
PinCnt=3
Pin="1",a,0,0,-3,-4
Pin="7",a,9,3,-2,-3
Pin="5",a,0,6,-3,18

[compdef]
Name=NFV
Definition=NFV
Shape=NFV
Mask=4864
memo=Analog behavioral voltage source (E.g. VALUE=I(R2)*V(3,4)^2)
Label Offset=18,12,16,13
PinCnt=2
Pin="Plus",6,0,-8,-4
Pin="Minus",0,0,-21,-6

[compdef]
Name=NFI
Definition=NFI
Shape=NFI
Mask=4096
memo=Analog behavioral current source (E.g. VALUE=Exp(-T/.5)*sin(2*PI*10*T))
Label Offset=15,12,-29,13
PinCnt=2
Pin="Plus",0,0,7,12
Pin="Minus",0,6,7,3

[Circuit]
Window Placement=2,3, -1,-1, -4,-23, 132,132,924,737
Default Object=Color=#000080
Default Object Font=Height=-15,FStyle=0,Color=#000080,Name=Arial
Default Object Apply Border To Text=No
Default Object Apply Fill To Text=No
WinBackGround Color=#FFFFFF
Select Color=#FF0000
Select Box Color=#000080
Grid Text Color=Height=-12,FStyle=0,Color=#FF0000,Name=Verdana
Component Color=#0000FF
Attribute Text=Height=-12,FStyle=0,Color=#008000,Name=Verdana
Wire Color=#008000
Bus Color=#008000
Pin Connection=Height=-10,FStyle=0,Color=#FF0000,Name=Arial
Node Number=Height=-11,FStyle=0,Color=#FF00FF,Name=Arial
Node Voltage Color=#000000
Dynamic AC Voltage Color=#E4E4E4
Text Banner Text=Height=-15,FStyle=0,Color=#800000,Name=Arial
Title Block Background=#C0C0C0
Current=Height=-11,FStyle=0,Color=#0000FF,Name=Arial
Power/Condition=Height=-11,FStyle=0,Color=#FF0000,Name=Arial
Digital Path Color=#FF0000
Title Block=Height=-15,FStyle=0,Color=#000000,Name=Arial
Disabled	Color=#C0C0C0
KeyWord Color=#0000FF
Error	Color=#FF0000
Digital 0 Color=#000000
Digital R Color=#FFFF00
Digital F Color=#FFFF00
Digital 1 Color=#FF0000
Digital X Color=#C0C0C0
Digital Z Color=#808080
SpiceType=AMBIGUOUS
Block Select Color=#51F998
TitleBlock Field_1=$name
TitleBlock Field_2=$user $company
TitleBlock Field_3
TitleBlock Field_4=$date
TitleBlock Field_5=Page $page of $maxpage
TitleBlock One Title=True
Title_Block_Border=False
Title_Block=False
Show Nodes=False
Show Voltages=False
Show Current=False
Show Power=False
Show Condition=False
Show Pin Connections=False
Show Cross=False
Show Attribute Text=True
Show Grid Text=True

[Comp]
Name=Battery
Grid=13,28
Rot=3

[Attr]
ONV=-29,-27,PART,Vin
Style=8192

[Attr]
ONV=-38,-41,VALUE,8.24
Style=8192

[Wire]
Grids=13,28,13,35

[Wire]
Grids=13,35,19,35

[Wire]
Grids=13,15,13,22

[Comp]
Name=Ground
Grid=13,35
Rot=1

[Comp]
Name=S (V-Switch)
Grid=31,21
Rot=3

[Attr]
ONV=14,-68,PART,S2
Style=8192

[Attr]
ONV=-29,-79,MODEL,SBREAK2

[Wire]
Grids=37,21,37,35

[Comp]
Name=Resistor
Grid=19,29
Rot=7

[Attr]
ONV=-32,11,PART,R27
Style=8192

[Attr]
ONV=-23,25,RESISTANCE,1k
Style=8192

[Wire]
Grids=19,35,27,35

[Comp]
Name=Fflop
Grid=27,29
Rot=5

[Attr]
ONV=-23,-39,PART,X11
Style=8192

[Attr]
ONV=-41,31,NAME,Fflop

[Wire]
Grids=27,21,28,21

[Wire]
Grids=13,15,31,15

[Wire]
Grids=28,21,31,21

[Wire]
Grids=19,21,19,29

[Wire]
Grids=19,21,24,21

[Comp]
Name=Voltage Source
Grid=27,35
Rot=3

[Attr]
ONV=16,-31,PART,Vclock
Style=8192

[Attr]
ONV=-200,-41,VALUE,PULSE 0 10 0 10n 10n 100n 5u

[Attr]
ONV=0,0,Saved_Pulse,DC 0 AC 1 0 Pulse 0 5 100n 10n 10n 400n 1u
Style=256

[Wire]
Grids=27,35,37,35

[Comp]
Name=OR2_CB
Grid=23,44
Rot=3

[Attr]
ONV=23,-30,PART,X13
Style=8192

[Attr]
ONV=-51,-28,NAME,OR2_CB

[Wire]
Grids=24,29,24,38

[Comp]
Name=Voltage Source
Grid=19,37
Rot=1

[Attr]
ONV=-56,17,PART,Vreset
Style=8192

[Attr]
ONV=15,27,VALUE,PULSE 0 10 4.8u 10n 10n 50n 5u

[Wire]
Grids=19,35,19,37

[Wire]
Grids=19,44,23,44

[Wire]
Grids=19,43,19,44

[Wire]
Grids=13,44,19,44

[Comp]
Name=Diode
Grid=43,22
Rot=7

[Attr]
ONV=-28,16,PART,D1
Style=8192

[Attr]
ONV=-61,26,MODEL,DBREAK

[Wire]
Grids=43,15,43,22

[Wire]
Grids=37,15,43,15

[Wire]
Grids=43,28,43,35

[Wire]
Grids=37,35,43,35

[Comp]
Name=Battery
Grid=51,15
Rot=6

[Attr]
ONV=-30,9,PART,VL
Style=8192

[Attr]
ONV=-27,21,VALUE,0

[Wire]
Grids=43,15,45,15

[Comp]
Name=Resistor
Grid=51,15

[Attr]
ONV=12,-35,PART,R5
Style=8192

[Attr]
ONV=12,-21,RESISTANCE,20m
Style=8192

[Comp]
Name=Inductor
Grid=63,15
Rot=6

[Attr]
ONV=-31,-38,PART,L1
Style=8192

[Attr]
ONV=-32,-24,INDUCTANCE,35u
Style=8192

[Wire]
Grids=63,15,65,15

[Wire]
Grids=75,15,84,15

[Comp]
Name=Resistor
Grid=65,18
Rot=7

[Attr]
ONV=-36,11,PART,Resr
Style=8192

[Attr]
ONV=-35,25,RESISTANCE,70m
Style=8192

[Comp]
Name=Capacitor
Grid=65,32
Rot=3

[Attr]
ONV=-42,-26,PART,Cout
Style=8192

[Attr]
ONV=-44,-40,CAPACITANCE,100u
Style=8192

[Wire]
Grids=65,15,65,18

[Wire]
Grids=65,24,65,26

[Wire]
Grids=65,32,65,35

[Wire]
Grids=43,35,65,35

[Wire]
Grids=65,15,75,15

[Comp]
Name=Resistor
Grid=75,22
Rot=7

[Attr]
ONV=-53,11,PART,Rupper
Style=8192

[Attr]
ONV=-69,25,RESISTANCE,{Rupper}
Style=8192

[Wire]
Grids=75,15,75,22

[Comp]
Name=S (V-Switch)
Grid=90,25
Rot=6

[Attr]
ONV=-72,9,PART,S1
Style=8192

[Attr]
ONV=-112,23,MODEL,SBREAK3

[Wire]
Grids=84,31,84,35

[Wire]
Grids=65,35,84,35

[Wire]
Grids=90,31,90,35

[Wire]
Grids=84,35,90,35

[Wire]
Grids=84,15,84,25

[Wire]
Grids=90,25,95,25

[Comp]
Name=Voltage Source
Grid=95,35
Rot=3

[Attr]
ONV=18,-32,PART,V13
Style=8192

[Attr]
ONV=-231,-41,VALUE,PWL 0 0 6m 0 6.1m 5 8m 5 8.1m 0

[Wire]
Grids=95,25,95,29

[Comp]
Name=Capacitor
Grid=58,40
Rot=4

[Attr]
ONV=16,11,PART,C2
Style=8192

[Attr]
ONV=8,26,CAPACITANCE,{C2}
Style=8192

[Comp]
Name=Capacitor
Grid=55,46
Rot=4

[Attr]
ONV=16,11,PART,C1
Style=8192

[Attr]
ONV=8,26,CAPACITANCE,{C1}
Style=8192

[Comp]
Name=Resistor
Grid=61,46

[Attr]
ONV=18,6,PART,R2
Style=8192

[Attr]
ONV=12,21,RESISTANCE,{R2}
Style=8192

[Comp]
Name=AMPSIMP
Grid=66,59
Rot=2

[Attr]
ONV=-35,-31,PART,X10
Style=8192

[Attr]
ONV=-87,-67,NAME,AMPSIMP

[Attr]
ONV=-298,-81,PARAMS:,Pole=10Meg Gain=30k Vhigh=5 Vlow=10m

[Comp]
Name=Battery
Grid=68,66
Rot=3

[Attr]
ONV=-35,-27,PART,Vref
Style=8192

[Attr]
ONV=-30,-41,VALUE,2.5
Style=8192

[Wire]
Grids=68,59,68,60

[Wire]
Grids=66,59,68,59

[Wire]
Grids=66,53,68,53

[Wire]
Grids=68,46,68,53

[Wire]
Grids=64,40,68,40

[Wire]
Grids=68,40,68,46

[Wire]
Grids=67,46,68,46

[Wire]
Grids=54,46,55,46

[Wire]
Grids=54,46,54,56

[Wire]
Grids=54,56,57,56

[Wire]
Grids=54,40,58,40

[Wire]
Grids=54,40,54,46

[Comp]
Name=Ground
Grid=68,66
Rot=7

[Comp]
Name=Resistor
Grid=75,60
Rot=1

[Attr]
ONV=8,11,PART,Rlower
Style=8192

[Attr]
ONV=8,25,RESISTANCE,10k
Style=8192

[Wire]
Grids=68,66,75,66

[Wire]
Grids=75,28,75,53

[Wire]
Grids=68,53,75,53

[Wire]
Grids=75,53,75,60

[Comp]
Name=NFV
Grid=25,50
Rot=3

[Attr]
ONV=-56,-39,PART,Ecomp
Style=8192

[Attr]
ONV=-145,-24,VALUE,If(V(Icoil, Err)>0,5,0 )
Style=8192

[Attr]
ONV=-61,-55,DERIVATIVE,Default

[Comp]
Name=Ground
Grid=25,50
Rot=7

[Wire]
Grids=51,56,54,56

[Comp]
Name=NFI
Grid=43,66
Rot=4

[Attr]
ONV=15,-26,PART,G1
Style=8192

[Attr]
ONV=15,-40,VALUE,If(V(LEB)>3,I(VL),0)
Style=8192

[Attr]
ONV=15,-54,DERIVATIVE,Default

[Wire]
Grids=43,66,68,66

[Comp]
Name=Resistor
Grid=38,60
Rot=7

[Attr]
ONV=-32,11,PART,R28
Style=8192

[Attr]
ONV=-16,25,RESISTANCE,1
Style=8192

[Wire]
Grids=38,60,43,60

[Wire]
Grids=38,66,43,66

[Comp]
Name=Capacitor
Grid=25,66
Rot=5

[Attr]
ONV=12,-26,PART,C3
Style=8192

[Attr]
ONV=12,-40,CAPACITANCE,100p
Style=8192

[Wire]
Grids=25,66,38,66

[Comp]
Name=Diode
Grid=21,54
Rot=1

[Attr]
ONV=14,9,PART,D2
Style=8192

[Attr]
ONV=12,24,MODEL,1N4148
Style=8192

[Attr]
ONV=12,54,PACKAGE,DO-35

[Wire]
Grids=21,60,25,60

[Wire]
Grids=25,60,30,60

[Comp]
Name=Resistor
Grid=16,54
Rot=7

[Attr]
ONV=-32,11,PART,R29
Style=8192

[Attr]
ONV=-23,25,RESISTANCE,1k
Style=8192

[Wire]
Grids=16,54,21,54

[Wire]
Grids=16,60,21,60

[Wire]
Grids=90,35,95,35

[Grid Text]
Text="senses theþinductor current"
Grid=45,21
Color=#000000
CBorder=NONE

[Grid Text]
Text="=R2"
Grid=42,48
Color=#000080
CBorder=NONE

[Grid Text]
Text="=C2"
Grid=42,46
Color=#000080
CBorder=NONE

[Grid Text]
Text="=C1"
Grid=42,44
Color=#000080
CBorder=NONE

[Grid Text]
Text="This is the cycle-by-cycle version of the averaged buckþconverter. Several elements have been added for thisþCM power supply.þ- X13 resets the latch and limits the max duty-cycle to 99%þ- G1 makes the floating coil current referenced to GNDþ- Ecomp is the peak current comparatorþ- the R29/D2/C3 generates a small delay for LEB actionþ- VL senses the inductor currentþþIn transient, plot V(Vout) and compare it to the signalþgiven by the averaged version of this CM buck."
Grid=11,88
CBorder=NONE

[Grid Text]
Text="The cycle-by-cycle CM simplified buck transient responseþRun Transient AnalysisþDesign by Christophe Basso"
Grid=12,10
FStyle=4
Color=#800000
CBorder=NONE

[Grid Text]
Text=".PARAM  C2={1/(2*pi*Fc*G*K*Rupper)} R2={K/(2*pi*Fc*C1)} G={10**(-(Gfc)/20)} þK={tan((boost/2+45)*pi/180)} boost={pm-(pfc)-90} C1={C2*(K**2-1)}"
Grid=11,96
Color=#800080
CBorder=NONE
Fill Pattern=Horizontal

[Grid Text]
Text=".PARAM  Gfc=-9.7 pfc=-75 Fc=5k Rupper=10k pm=45 "
Grid=11,92
Color=#800080
CBorder=NONE
Fill Pattern=Horizontal

[Grid Text]
Text="Q"
Grid=28,21
CBorder=NONE

[Grid Text]
Text="Reset"
Grid=13,44
CBorder=NONE

[Grid Text]
Text="Vout"
Grid=75,15
CBorder=NONE

[Grid Text]
Text="Err"
Grid=51,56
CBorder=NONE

[Grid Text]
Text="Icoil"
Grid=38,60
CBorder=NONE

[Grid Text]
Text="LEB"
Grid=30,60
CBorder=NONE

[Grid Text]
Text="Q"
Grid=16,54
CBorder=NONE

[Schematic]
CurrentSection 0=0
CurrentSection 1=0
CurrentSection 2=0
CurrentSection 3=0
Splitter.xs=0
Splitter.ys=0
TextQuad=4099
Scale=1
PrinterScale=1
GridUser=10
ShapeGroups="Main","Euro","DeMorgan","Polarity","Electrolytic"
CalcRMS=False
CalcAVG=False
CalcPeak=False
DisplayMeasure=Last

[Tools]
Pos=Top
PROBE=Yes
SELECT=Yes
COMP=Yes
TEXT=Yes
WIRE=Yes
WIRED=Yes
BUS=Yes
GRAPHIC=Yes
LINE=No
ELLIPSE=No
RECT=No
DIAM=No
ARC=No
PIE=No
LEFTBRK=No
RIGHTBRK=No
BOTHBRK=No
FLAG=Yes
META=No
INFO=Yes
HELP=Yes
LINK=Yes
REGION_ENABLE=Yes
DIGTRC=No
DIGTRC2=No
DIGALL=No
GRIDTEXT=Yes
COMPTEXT=Yes
NODE=Yes
MEASURED=Yes
NODEV=Yes
CURRENT=Yes
POWER=Yes
CONDITIN=Yes
PIN=Yes
CROSS=No
GRID=Yes
BORDER=No
TITLE=Yes
RUBBER=Yes
PROPERTY=Yes
STEP=Yes
MIRROR=Yes
ROTATE=Yes
FLIPY=Yes
FLIPX=Yes
FINDCOMP=Yes
FIND=Yes
REPEAT=No
MODEL=Yes
CIR2CKT=No
ATTDISP=No
ENABLE=Yes
DISABLE=Yes
TOFRONT=Yes
TOBACK=Yes
SELNEXT=No
PAGEADD=No
PAGEDEL=No
ZOOMIN=Yes
ZOOMOUT=Yes
GOTOFLAG=No
UPLEVEL=Yes
COLOR=Yes
FONT=Yes

[Section]
Index=0
Name="Test Buck Cycle-by-Cycle CM"
Type=Main
Enable=True
CurrentPage 0=0
CurrentPage 1=0
CurrentPage 2=0
CurrentPage 3=0
TabSize 0=400
TabSize 1=400
TabSize 2=400
TabSize 3=400

[Page]
Index=0
Section=0
Print=True
Enable=True
Name=Main
Scale 0=1
Scale 1=1
Scale 2=1
Scale 3=1
Grid=88,46

[Page]
Index=1
Section=0
Type=Text
Print=False
Enable=True
Name=Text

[Page]
Index=2
Section=0
Type=Text
Print=False
Enable=True
Name=Models

[Page]
Index=3
Section=0
Type=Info
Print=False
Enable=True
Name=Info

[Text Area]
Section=0
Page=1
Font=Height=-15,FStyle=0,Color=#000000,Name=Courier New
Comment Color=#008000
Background Color=#FFFFFF
Len=22
.options method=gear


[Text Area]
Section=0
Page=2
Font=Height=-15,FStyle=0,Color=#000000,Name=Courier New
Comment Color=#008000
Background Color=#FFFFFF
Len=147
.MODEL 1N4148 D (BV=100 CJO=1.337036P IBV=100.000001P IS=7.187424N
+ M=316.713486M N=1.94878 RL=3.521383G RS=439.577908M TT=8.952928N VJ=9.476621)

[Transient]
Font=Height=-15,FStyle=0,Color=#0000FF,Name=Arial
WinBackGround Color=#FFFFFF
Select Color=#FF0000
Select Box Color=#000080
Title=Test Buck Closed Loop CM.cir
AutoTitle=Yes
Grid Color=#808080
Grid Weight=1
Grid Pattern=Dot6
Tracker Foreground=Height=-15,FStyle=0,Color=#000000,Name=Arial
Tracker Background=#FFFF00
Baseline color=#0000FF
Static Grids=False
PlusMark=False
MinorLog25=Off
LabelMinor=Off
OperPoint=True
OperPointOnly=False
AutoScaleRanges=False
DataPoints=False
Token=False
Ruler=False
XAxisGrids=True
YAxisGrids=True
MinorLogGrids=True
BaseLine=False
Graph Background=#FFFFFF
Tracker Intercept=False
Tracker Mouse=True
Tracker Cursor=True
Tracker Cursor BranchInfo=False
Horizontal Cursor=False
Same Y Scales=Yes
Enable X Scaling=True
Enable Y Scaling=True
Keep X Scales The Same=False
Number of Grids X=5
Number of Grids Y=5
Cursor Select Color Primary=#C0C0C0
Cursor Select Color Secondary=#FF0000
Data Point Labels Color Fore=Height=-15,FStyle=0,Color=#000000,Name=Arial
Data Point Labels Color Back=#FFFF00
FFT_NPts="1024"
FFT_IncludeDCHarmonic=False
FFT_AutoScale_Harmonics="10"
PrinterAutoTile=No
PrinterBlackBorder=No
MonMaxShow=2
MonPageWidth=66
MonPlotWidth=21
MonExprXWidth=142
MonExprYWidth=260
MonRangeXWidth=90
MonRangeYWidth=90
AnimateWait=0
AnimateWaitTime=500
Save_For_Future=No
Reduce_Display=1
Reduce_Save=1
Num Out Header Left
Num Out Header Center="$MC\n$user\n$company\n$Analysis of $name"
Num Out Header Right
Num Out Delimiter=32
Num Out Write=True
Num Out Write Main Header=True
Num Out Write Limits=True
Num Out Write Branch Header=True
Num Out Write Models=True
Num Out Write Zero Models=True
Num Out Write Undefined Models=True
Num Out Write Operating Point=True
Num Out Write Values=True
Num Out Write Waveform Header=True
Num Out Low="TMIN"
Num Out High="TMAX"
Num Out Font=Height=-15,FStyle=0,Color=#000080,Name=Courier New

[Tools]
Pos=Top
SELECT=Yes
GRAPHIC=Yes
LINE=No
ELLIPSE=No
RECT=No
DIAM=No
ARC=No
PIE=No
LEFTBRK=No
RIGHTBRK=No
BOTHBRK=No
POLYCLOS=No
SCALE=Yes
CURSOR=Yes
MEASUREH=Yes
MEASUREV=Yes
TAG=Yes
PTAG=Yes
TEXT=Yes
PROPERTY=Yes
START=Yes
STOP=Yes
PAUSE=Yes
DATAPTS=Yes
TOKENS=Yes
RULER=Yes
PLUS=Yes
XAXIS=Yes
YAXIS=Yes
MINORLOG=Yes
LOG25=Yes
BASELINE=Yes
HORIZCUR=Yes
GOTOX=Yes
GOTOY=Yes
GOTOPERF=Yes
GOTOBRNC=Yes
CLEAR_ACCUMULATED=Yes
PDELETE_ALL_PLOTS=Yes
NEXT=Yes
NEXTIN=Yes
PEAK=Yes
VALLEY=Yes
HIGH=Yes
LOW=Yes
INFLECTN=Yes
GHIGH=Yes
GLOW=Yes
BOTTOM=Yes
TOP=Yes
WAVEFORMBUFFER=Yes
AOUTPUT=Yes
PKEY=Yes
ENXSCALE=Yes
ENYSCALE=Yes
ZOOMIN=Yes
ZOOMOUT=Yes
AUTOSCALE=No
COLOR=Yes
FONT=Yes
SELNEXT=No

[APage]
Analysis=Transient
Name="Main"

[AC]
Font=Height=-15,FStyle=0,Color=#0000FF,Name=Arial
WinBackGround Color=#FFFFFF
Select Color=#FF0000
Select Box Color=#000080
Title
AutoTitle=Yes
Grid Color=#808080
Grid Weight=1
Grid Pattern=Dot6
Tracker Foreground=Height=-15,FStyle=0,Color=#000000,Name=Arial
Tracker Background=#FFFF00
Baseline color=#0000FF
Static Grids=False
PlusMark=False
MinorLog25=Off
LabelMinor=Off
OperPoint=True
OperPointOnly=False
AutoScaleRanges=False
DataPoints=False
Token=False
Ruler=False
XAxisGrids=True
YAxisGrids=True
MinorLogGrids=True
BaseLine=False
Graph Background=#FFFFFF
Tracker Intercept=False
Tracker Mouse=True
Tracker Cursor=True
Tracker Cursor BranchInfo=False
Horizontal Cursor=False
Same Y Scales=Yes
Enable X Scaling=True
Enable Y Scaling=True
Keep X Scales The Same=False
Number of Grids X=5
Number of Grids Y=5
Cursor Select Color Primary=#C0C0C0
Cursor Select Color Secondary=#FF0000
Data Point Labels Color Fore=Height=-15,FStyle=0,Color=#000000,Name=Arial
Data Point Labels Color Back=#FFFF00
FFT_NPts="1024"
FFT_IncludeDCHarmonic=False
FFT_AutoScale_Harmonics="10"
PrinterAutoTile=No
PrinterBlackBorder=No
MonMaxShow=3
MonPageWidth=66
MonPlotWidth=21
MonExprXWidth=142
MonExprYWidth=260
MonRangeXWidth=90
MonRangeYWidth=90
AnimateWait=0
AnimateWaitTime=500
Save_For_Future=No
Reduce_Display=1
Reduce_Save=1
Num Out Header Left
Num Out Header Center="$MC\n$user\n$company\n$Analysis of $name"
Num Out Header Right
Num Out Delimiter=32
Num Out Write=True
Num Out Write Main Header=True
Num Out Write Limits=True
Num Out Write Branch Header=True
Num Out Write Models=True
Num Out Write Zero Models=True
Num Out Write Undefined Models=True
Num Out Write Operating Point=True
Num Out Write Noise=True
Num Out Write Values=True
Num Out Write Waveform Header=True
Num Out Low="FMIN"
Num Out High="FMAX"
Num Out Font=Height=-15,FStyle=0,Color=#000080,Name=Courier New

[Tools]
Pos=Top
SELECT=Yes
GRAPHIC=Yes
LINE=No
ELLIPSE=No
RECT=No
DIAM=No
ARC=No
PIE=No
LEFTBRK=No
RIGHTBRK=No
BOTHBRK=No
POLYCLOS=No
SCALE=Yes
CURSOR=Yes
MEASUREH=Yes
MEASUREV=Yes
TAG=Yes
PTAG=Yes
TEXT=Yes
PROPERTY=Yes
START=Yes
STOP=Yes
PAUSE=Yes
DATAPTS=Yes
TOKENS=Yes
RULER=Yes
PLUS=Yes
XAXIS=Yes
YAXIS=Yes
MINORLOG=Yes
LOG25=Yes
BASELINE=Yes
HORIZCUR=Yes
GOTOX=Yes
GOTOY=Yes
GOTOPERF=Yes
GOTOBRNC=Yes
CLEAR_ACCUMULATED=Yes
PDELETE_ALL_PLOTS=Yes
NEXT=Yes
NEXTIN=Yes
PEAK=Yes
VALLEY=Yes
HIGH=Yes
LOW=Yes
INFLECTN=Yes
GHIGH=Yes
GLOW=Yes
BOTTOM=Yes
TOP=Yes
WAVEFORMBUFFER=Yes
AOUTPUT=Yes
PKEY=Yes
ENXSCALE=Yes
ENYSCALE=Yes
ZOOMIN=Yes
ZOOMOUT=Yes
AUTOSCALE=No
COLOR=Yes
FONT=Yes
SELNEXT=No

[APage]
Analysis=AC
Name="Main"

[Monte Carlo Options]
Analysis=Transient
Status=Off
Zero Tolerance=False
Distribution=Normal
Number of Runs=10
Seed=0

[Monte Carlo Options]
Analysis=AC
Status=Off
Zero Tolerance=False
Distribution=Normal
Number of Runs=10
Seed=0

[Limits]
Analysis=Transient
TRange=10m
TStep=250n
NPts=51
Temp=27
RetraceRuns=1
StateVar=Zero
RunOption=Normal
Temperature Type=Linear
Accumulate Plots=False

[WaveForm]
Analysis=Transient
Plt=1
AliasID=1
XExp=T
YExp=V(Vout)
XRng=10m,5m
YRng=5.03,4.97
Options=LINEARX,LINEARY
Range Grid X=1m
Range Grid Y=.01
CS=Normal
Line Color=#FF0000
Text Color=#FF0000
Rainbow=False
VFmtX=3
VFmtY=3
ScaleFactorX="None"
ScaleFactorY="None"
ScaleUnitsX="Auto"
ScaleUnitsY="Auto"
SFmtX=3
SFmtY=3

[WaveForm]
Analysis=Transient
AliasID=-1
Options=LINEARX,LINEARY
Line Color=#008000
Text Color=#008000
Rainbow=False
VFmtX=3
VFmtY=3
ScaleFactorX="None"
ScaleFactorY="None"
ScaleUnitsX="Auto"
ScaleUnitsY="Auto"
SFmtX=3
SFmtY=3

[Limits]
Analysis=AC
FRange=1E8,1Meg
NPts=51
Temp=27
MaxChng=5
NInput=NONE
NOutput=2
Sweep type=Auto
StateVar=Zero
RunOption=Normal
Temperature Type=Linear
Accumulate Plots=False

[WaveForm]
Analysis=AC
Plt=1
AliasID=1
XExp=F
YExp=db(v(ERR))
XRng=1e8,1e6
YRng=-2000
Options=LINEARY
Range Grid X=1.98e7
Range Grid Y=400
Line Color=#0000FF
Text Color=#0000FF
Rainbow=False
VFmtX=3
VFmtY=3
ScaleFactorX="None"
ScaleFactorY="None"
ScaleUnitsX="Auto"
ScaleUnitsY="Auto"
SFmtX=3
SFmtY=3

[WaveForm]
Analysis=AC
Plt=2
AliasID=2
XExp=F
YExp=ph(v(ERR))
XRng=1e8,1e6
YRng=1,-1
Options=LINEARY
Range Grid X=1.98e7
Range Grid Y=0.5
Line Color=#FF0000
Text Color=#FF0000
Rainbow=False
VFmtX=3
VFmtY=3
ScaleFactorX="None"
ScaleFactorY="None"
ScaleUnitsX="Auto"
ScaleUnitsY="Auto"
SFmtX=3
SFmtY=3

[WaveForm]
Analysis=AC
AliasID=-1
Options=LINEARY
Line Color=#008000
Text Color=#008000
Rainbow=False
VFmtX=3
VFmtY=3
ScaleFactorX="None"
ScaleFactorY="None"
ScaleUnitsX="Auto"
ScaleUnitsY="Auto"
SFmtX=3
SFmtY=3

[Limits]
Analysis=DynamicAC
FirstValueDisplay=Mag
SecondValueDisplay=PhaseDeg
PlaceText=True

[Limits]
Analysis=DynamicDC
PlaceText=True

[Pane]
Analysis=Transient
CurrentPage 0="Main"

[Pane]
Analysis=AC
CurrentPage 0="Main"

[Pane]
Analysis=DC

[Pane]
Analysis=Distortion

[Watch]
Analysis=Transient
Format=3
ExprPercentWidth=80

[Watch]
Analysis=AC
Format=3
ExprPercentWidth=80

[OPMethods]
Analysis=Transient
Standard Newton-Raphson=0,0
Source Stepping=0,0
Diagonal Gmin Stepping=0,0
Junction Gmin Stepping=0,0
Pseudo Transient=0,0

[OPMethods]
Analysis=AC
Standard Newton-Raphson=0,0
Source Stepping=0,0
Diagonal Gmin Stepping=0,0
Junction Gmin Stepping=0,0
Pseudo Transient=0,0

[OPMethods]
Analysis=DC
Standard Newton-Raphson=0,0
Source Stepping=0,0
Diagonal Gmin Stepping=0,0
Junction Gmin Stepping=0,0
Pseudo Transient=0,0
